"OH015"|7|"DEP"|"Depression, closed"|A shallow, saucer-shaped area that is slightly lower on the landscape than the surrounding area and that does not have a natural outlet for surface drainage. Typically .2 to 2 acres.|"253883"
"OH015"|7|"ERO"|"Severely eroded spot"|An area where on the average 75 percent or more of the original surface layer has been lost because of accelerated erosion. Not used in map units that are named severely eroded, very severely eroded, or gullied. Typically .2 to 2 acres.|"253884"
"OH015"|7|"ESO"|"Escarpment, nonbedrock"|A relatively continuous and steep slope or cliff, which generally is produced by erosion but can be produced by faulting, that breaks the continuity of more gently sloping land surfaces. Exposed earthy material is non soil or very shallow soil.|"253885"
"OH015"|7|"GPI"|"Gravel pit"|An open excavation from which soil and underlying material have been removed and used, without crushing, as a source of sand or gravel. Typically .2 to 2 acres.|"253886"
"OH015"|7|"GRA"|"Gravelly spot"|A spot where the surface layer has more than 35 percent, by volume, rock fragments that are mostly less than 3 inches in diameter in an area that has less than 15 percent rock fragments. Typically .2 to 2 acres.|"253887"
"OH015"|7|"SLP"|"Short, steep slope"|A narrow area of soil having slopes that are at least two slope classes steeper than the slope class of the surrounding map unit.|"253888"
"OH015"|7|"TYP"|"Typical pedon site"|Site of the pedon described as typical for series in the county.|"253889"
"OH015"|7|"WAT"|"Perennial water"|Small, natural or constructed lakes, ponds, or pits that contain water most of the year. Typically .2 to 2 acres.|"253890"
"OH015"|7|"WET"|"Wet spot"|A somewhat poorly drained to very poorly drained area that is at least two drainage classes wetter than the named soils in the surrounding map unit. Typically .2 to 2 acres.|"253891"
