<!DOCTYPE qgis PUBLIC 'http://mrcc.com/qgis.dtd' 'SYSTEM'>
<qgis version="3.36.1-Maidenhead">
  <identifier>MUPOLYGON</identifier>
  <parentidentifier></parentidentifier>
  <language>ENG</language>
  <type>dataset</type>
  <title>MUPOLYGON - Ohio</title>
  <abstract>This dataset is a digital soil survey and generally is the most detailed level of soil geographic data developed by the National Cooperative Soil Survey. The information was prepared by digitizing maps, by compiling information onto a planimetric correct base and digitizing, or by revising digitized maps using remotely sensed and other information.This dataset consists of georeferenced digital map data and computerized attribute data. The map data are in a state-wide extent format and include a detailed, field verified inventory of soils and miscellaneous areas that normally occur in a repeatable pattern on the landscape and that can be cartographically shown at the scale mapped. The soil map units are linked to attributes in the National Soil Information System relational database, which gives the proportionate extent of the component soils and their properties.

The dataset was created for use in national, regional, and state-wide resource planning and analysis of soils data. The Soil Survey Geographic (SSURGO) Database depicts information about the kinds and distribution of soils on the landscape. The soil map and data used in the SSURGO product were prepared by soil scientists as part of the National Cooperative Soil Survey.</abstract>
  <keywords vocabulary="Search keys">
    <keyword>Soil Survey</keyword>
    <keyword>Ohio</keyword>
    <keyword>GDG</keyword>
    <keyword>geoscientificInformation</keyword>
    <keyword>OH007 (2023-08-31), OH085 (2023-09-07), OH171 (2023-09-11), OH051 (2023-09-06), OH095 (2023-09-07), OH123 (2023-09-11), OH055 (2023-09-06), OH173 (2023-09-11), OH043 (2023-09-06), OH035 (2023-09-06), OH069 (2023-09-06), OH143 (2023-09-11), OH093 (2023-09-07), OH155 (2023-09-11), OH039 (2023-09-06), OH153 (2023-09-11), OH125 (2023-09-11), OH147 (2023-09-11), OH077 (2023-09-06), OH103 (2023-09-07), OH133 (2023-09-11), OH137 (2023-09-11), OH063 (2023-09-06), OH005 (2023-08-31), OH099 (2023-09-07), OH161 (2023-09-11), OH175 (2023-09-11), OH033 (2023-08-31), OH139 (2023-09-11), OH169 (2023-09-11), OH151 (2023-09-11), OH003 (2023-09-06), OH029 (2023-08-31), OH065 (2023-09-06), OH107 (2023-09-07), OH011 (2023-08-31), OH101 (2023-09-07), OH117 (2023-09-08), OH075 (2023-09-08), OH157 (2023-09-11), OH019 (2023-08-31), OH083 (2023-09-07), OH081 (2023-09-06), OH149 (2023-09-11), OH091 (2023-09-07), OH159 (2023-09-11), OH031 (2023-08-31), OH037 (2023-09-06), OH041 (2023-09-06), OH067 (2023-09-06), OH021 (2023-08-31), OH089 (2023-09-07), OH109 (2023-09-08), OH119 (2023-09-08), OH059 (2023-09-06), OH013 (2023-08-31), OH097 (2023-09-07), OH049 (2023-09-06), OH023 (2023-08-31), OH121 (2023-09-11), OH135 (2023-09-11), OH113 (2023-09-08), OH057 (2023-09-07), OH045 (2023-09-06), OH127 (2023-09-11), OH111 (2023-09-08), OH129 (2023-09-11), OH115 (2023-09-08), OH047 (2023-09-06), OH073 (2023-09-06), OH017 (2023-08-31), OH165 (2023-09-11), OH027 (2023-08-31), OH009 (2023-08-31), OH167 (2023-09-11), OH141 (2023-09-11), OH071 (2023-09-06), OH163 (2023-09-11), OH061 (2023-09-06), OH025 (2023-08-31), OH015 (2023-08-31), OH131 (2023-09-11), OH079 (2023-09-06), OH105 (2023-09-07), OH001 (2023-08-31), OH145 (2023-09-12), OH053 (2023-09-06), OH087 (2023-09-07)</keyword>
    <keyword>farming</keyword>
    <keyword>soils</keyword>
    <keyword>gSSURGO</keyword>
    <keyword>Geospatial Data Gateway</keyword>
    <keyword>SSURGO</keyword>
    <keyword>United States of America</keyword>
    <keyword>environment</keyword>
    <keyword>USA</keyword>
  </keywords>
  <keywords vocabulary="gmd:topicCategory">
    <keyword>geoscientificInformation</keyword>
    <keyword>farming</keyword>
    <keyword>environment</keyword>
    <keyword>Soil Survey</keyword>
    <keyword>GDG</keyword>
    <keyword>soils</keyword>
    <keyword>gSSURGO</keyword>
    <keyword>Geospatial Data Gateway</keyword>
    <keyword>SSURGO</keyword>
  </keywords>
  <contact>
    <contactAddress>
      <type>postal</type>
      <address>Federal Building, Room 152</address>
      <city>Lincoln</city>
      <administrativearea>NE</administrativearea>
      <postalcode>68508-3866</postalcode>
      <country>US</country>
    </contactAddress>
    <name></name>
    <organization>U.S. Department of Agriculture, Natural Resources Conservation Service, National Soil Survey Center</organization>
    <position></position>
    <voice></voice>
    <fax></fax>
    <email>SoilsHotline@usda.gov</email>
    <role>Point of contact</role>
  </contact>
  <links>
    <link format="" type="" description="" url="http://datagateway.nrcs.usda.gov" size="" name="ESRI File Geodatabase" mimeType=""/>
  </links>
  <dates/>
  <fees></fees>
  <constraints type="Limitations of use">The U.S. Department of Agriculture, Natural Resources Conservation Service, should be acknowledged as the data source in products derived from these data.This dataset is not designed for use as a primary regulatory tool in permitting or siting decisions, but may be used as a reference source. This is public information and may be interpreted by organizations, agencies, units of government, or others based on needs; however, they are responsible for the appropriate application. Federal, State, or local regulatory bodies are not to reassign to the Natural Resources Conservation Service any authority for the decisions that they make. The Natural Resources Conservation Service will not perform any evaluations of these maps for purposes related solely to State or local regulatory programs. Digital data files are periodically updated. Files are dated, and users are responsible for obtaining the latest version of the data.</constraints>
  <rights>Soil Survey Staff. Gridded Soil Survey Geographic (gSSURGO) Database for Ohio. United States Department of Agriculture, Natural Resources Conservation Service. Available online at http://datagateway.nrcs.usda.gov/. 20230912 (202310 official release).</rights>
  <encoding></encoding>
  <crs>
    <spatialrefsys nativeFormat="Wkt">
      <wkt>PROJCRS["NAD83 / Conus Albers",BASEGEOGCRS["NAD83",DATUM["North American Datum 1983",ELLIPSOID["GRS 1980",6378137,298.257222101,LENGTHUNIT["metre",1]]],PRIMEM["Greenwich",0,ANGLEUNIT["degree",0.0174532925199433]],ID["EPSG",4269]],CONVERSION["Conus Albers",METHOD["Albers Equal Area",ID["EPSG",9822]],PARAMETER["Latitude of false origin",23,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8821]],PARAMETER["Longitude of false origin",-96,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8822]],PARAMETER["Latitude of 1st standard parallel",29.5,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8823]],PARAMETER["Latitude of 2nd standard parallel",45.5,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8824]],PARAMETER["Easting at false origin",0,LENGTHUNIT["metre",1],ID["EPSG",8826]],PARAMETER["Northing at false origin",0,LENGTHUNIT["metre",1],ID["EPSG",8827]]],CS[Cartesian,2],AXIS["easting (X)",east,ORDER[1],LENGTHUNIT["metre",1]],AXIS["northing (Y)",north,ORDER[2],LENGTHUNIT["metre",1]],USAGE[SCOPE["Data analysis and small scale data presentation for contiguous lower 48 states."],AREA["United States (USA) - CONUS onshore - Alabama; Arizona; Arkansas; California; Colorado; Connecticut; Delaware; Florida; Georgia; Idaho; Illinois; Indiana; Iowa; Kansas; Kentucky; Louisiana; Maine; Maryland; Massachusetts; Michigan; Minnesota; Mississippi; Missouri; Montana; Nebraska; Nevada; New Hampshire; New Jersey; New Mexico; New York; North Carolina; North Dakota; Ohio; Oklahoma; Oregon; Pennsylvania; Rhode Island; South Carolina; South Dakota; Tennessee; Texas; Utah; Vermont; Virginia; Washington; West Virginia; Wisconsin; Wyoming."],BBOX[24.41,-124.79,49.38,-66.91]],ID["EPSG",5070]]</wkt>
      <proj4>+proj=aea +lat_0=23 +lon_0=-96 +lat_1=29.5 +lat_2=45.5 +x_0=0 +y_0=0 +ellps=GRS80 +towgs84=0,0,0,0,0,0,0 +units=m +no_defs</proj4>
      <srsid>28001</srsid>
      <srid>5070</srid>
      <authid>EPSG:5070</authid>
      <description>NAD83 / Conus Albers</description>
      <projectionacronym>aea</projectionacronym>
      <ellipsoidacronym>EPSG:7019</ellipsoidacronym>
      <geographicflag>false</geographicflag>
    </spatialrefsys>
  </crs>
  <extent>
    <spatial maxy="42.41149000000000058" minz="0" crs="EPSG:5070" miny="38.22602100000000291" maxx="-80.22785000000000366" maxz="0" minx="-85.27113599999999849" dimensions="2"/>
  </extent>
</qgis>
